<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<schematic>
<libraries>
<library name="ALPS Dual Library">
<description>Upverter Parts Library

Created by Upverter.com</description>
<packages>
<package name="ALPS_EC11EBB24C03_0">
<description>Compact and highly reliable type available in many varieties</description>
</package>
</packages>
<symbols>
<symbol name="ALPS_EC11EBB24C03_0_0">
<description>Compact and highly reliable type available in many varieties</description>
<pin name="MNT_1"/>
<pin name="MNT_2"/>
<pin name="A"/>
<pin name="A'"/>
<pin name="B"/>
<pin name="B'"/>
<pin name="C"/>
<pin name="C'"/>
<pin name="D"/>
<pin name="E"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ALPS_EC11EBB24C03" prefix="ENC">
<description>Compact and highly reliable type available in many varieties</description>
<gates>
<gate name="G$0" symbol="ALPS_EC11EBB24C03_0_0"/>
</gates>
<devices>
<device name="ALPS_EC11EBB24C03_0_0" package="ALPS_EC11EBB24C03_0">
<connects>
<connect gate="G$0" pin="A" pad="8"/>
<connect gate="G$0" pin="A'" pad="1"/>
<connect gate="G$0" pin="B" pad="10"/>
<connect gate="G$0" pin="B'" pad="3"/>
<connect gate="G$0" pin="C" pad="9"/>
<connect gate="G$0" pin="C'" pad="2"/>
<connect gate="G$0" pin="D" pad="4"/>
<connect gate="G$0" pin="E" pad="5"/>
<connect gate="G$0" pin="MNT_1" pad="6"/>
<connect gate="G$0" pin="MNT_2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="DATASHEET" value="http://www.alps.com/prod/info/E/HTML/Encoder/Incremental/EC11/EC11EBB24C03.html"/>
<attribute name="DIGIKEY_DESCRIPTION" value="ENC "/>
<attribute name="LEAD_FREE" value="yes"/>
<attribute name="MF" value="ALPS"/>
<attribute name="MOUNTING_STYLE" value="PCB Mount"/>
<attribute name="MOUSER_PART_NUMBER" value="688-EC11EBB24C03"/>
<attribute name="MPN" value="EC11EBB24C03"/>
<attribute name="NUMBER_OF_CHANNELS" value="2 Channel"/>
<attribute name="NUMBER_OF_DETENTS" value="30 Detent"/>
<attribute name="OPERATING_LIFE_(CYCLES)" value="15000"/>
<attribute name="OUTPUT_TYPE" value="Quadrature"/>
<attribute name="PACKAGE" value="ENCODER_PTH_11MM7X12MM0"/>
<attribute name="PREFIX" value="ENC"/>
<attribute name="RATING" value="10mA 5VDC"/>
<attribute name="RESOLUTION" value="15 PPR"/>
<attribute name="ROHS" value="yes"/>
<attribute name="TECHNOLOGY" value="Rotary"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+85°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-40°C"/>
<attribute name="TERMINATION_STYLE" value="Through Hole"/>
<attribute name="TYPE" value="Incremental"/>
<attribute name="VOLTAGE" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="SparkFun-Boards_WITH_CAD">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
This library contains footprints for SparkFun breakout boards, microcontrollers (Arduino, Particle, Teensy, etc.),  breadboards, non-RF modules, etc.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ARDUINO_MEGA">
<description>&lt;h3&gt; Arduino MEGA R3 footprint&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:82&lt;/li&gt;
&lt;li&gt;Area:4x2.15 in&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;

&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Arduino Mega R3&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
<symbols>
</symbols>
<devicesets>
</devicesets>
</library>
<library name="SnapEDA Library">
<packages>
<package name="MODULE_MEGA_PRO_EMBED_CH340G_/_ATMEGA2560">
</package>
<package name="SW_482016514001">
</package>
</packages>
<symbols>
<symbol name="MEGA_PRO_EMBED_CH340G_/_ATMEGA2560">
<pin name="AREF"/>
<pin name="RX" direction="in"/>
<pin name="D2"/>
<pin name="D4"/>
<pin name="D6"/>
<pin name="D8"/>
<pin name="D10"/>
<pin name="D12"/>
<pin name="D14"/>
<pin name="D16"/>
<pin name="D18"/>
<pin name="D20"/>
<pin name="D22"/>
<pin name="D24"/>
<pin name="D26"/>
<pin name="D28"/>
<pin name="D30"/>
<pin name="VIN" direction="sup"/>
<pin name="GND" direction="pwr"/>
<pin name="5V" direction="pwr"/>
<pin name="3V3" direction="pwr"/>
<pin name="RST" direction="in"/>
<pin name="TX" direction="out"/>
<pin name="D3"/>
<pin name="D5"/>
<pin name="D7"/>
<pin name="D9"/>
<pin name="D11"/>
<pin name="D13"/>
<pin name="D15"/>
<pin name="D17"/>
<pin name="D19"/>
<pin name="D21"/>
<pin name="D23"/>
<pin name="D25"/>
<pin name="D27"/>
<pin name="D29"/>
<pin name="D31"/>
<pin name="D33"/>
<pin name="D35"/>
<pin name="D37"/>
<pin name="D39"/>
<pin name="D41"/>
<pin name="D43"/>
<pin name="D45"/>
<pin name="D47"/>
<pin name="D49"/>
<pin name="D51"/>
<pin name="D53"/>
<pin name="A1"/>
<pin name="A3"/>
<pin name="A5"/>
<pin name="A7"/>
<pin name="D32"/>
<pin name="D34"/>
<pin name="D36"/>
<pin name="D38"/>
<pin name="D40"/>
<pin name="D42"/>
<pin name="D44"/>
<pin name="D46"/>
<pin name="D48"/>
<pin name="D50"/>
<pin name="D52"/>
<pin name="A0"/>
<pin name="A2"/>
<pin name="A4"/>
<pin name="A6"/>
<pin name="A8"/>
<pin name="A9"/>
<pin name="A11"/>
<pin name="A13"/>
<pin name="A15"/>
<pin name="A10"/>
<pin name="A12"/>
<pin name="A14"/>
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="SCK" function="clk"/>
<pin name="RESET" direction="in"/>
</symbol>
<symbol name="482016514001">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MEGA_PRO_EMBED_CH340G_/_ATMEGA2560" prefix="U">
<description>Mega 2560 PRO (Embed) CH340G/ATmega2560-16AU  </description>
<gates>
<gate name="G$1" symbol="MEGA_PRO_EMBED_CH340G_/_ATMEGA2560"/>
</gates>
<devices>
<device name="" package="MODULE_MEGA_PRO_EMBED_CH340G_/_ATMEGA2560">
<connects>
<connect gate="G$1" pin="3V3" pad="3V3_1 3V3_2"/>
<connect gate="G$1" pin="5V" pad="5V_1 5V_2 5V_3"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A12" pad="A12"/>
<connect gate="G$1" pin="A13" pad="A13"/>
<connect gate="G$1" pin="A14" pad="A14"/>
<connect gate="G$1" pin="A15" pad="A15"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D10" pad="D10"/>
<connect gate="G$1" pin="D11" pad="D11"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D14" pad="D14"/>
<connect gate="G$1" pin="D15" pad="D15"/>
<connect gate="G$1" pin="D16" pad="D16"/>
<connect gate="G$1" pin="D17" pad="D17"/>
<connect gate="G$1" pin="D18" pad="D18"/>
<connect gate="G$1" pin="D19" pad="D19"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D20" pad="D20"/>
<connect gate="G$1" pin="D21" pad="D21"/>
<connect gate="G$1" pin="D22" pad="D22"/>
<connect gate="G$1" pin="D23" pad="D23"/>
<connect gate="G$1" pin="D24" pad="D24"/>
<connect gate="G$1" pin="D25" pad="D25"/>
<connect gate="G$1" pin="D26" pad="D26"/>
<connect gate="G$1" pin="D27" pad="D27"/>
<connect gate="G$1" pin="D28" pad="D28"/>
<connect gate="G$1" pin="D29" pad="D29"/>
<connect gate="G$1" pin="D3" pad="D3"/>
<connect gate="G$1" pin="D30" pad="D30"/>
<connect gate="G$1" pin="D31" pad="D31"/>
<connect gate="G$1" pin="D32" pad="D32"/>
<connect gate="G$1" pin="D33" pad="D33"/>
<connect gate="G$1" pin="D34" pad="D34"/>
<connect gate="G$1" pin="D35" pad="D35"/>
<connect gate="G$1" pin="D36" pad="D36"/>
<connect gate="G$1" pin="D37" pad="D37"/>
<connect gate="G$1" pin="D38" pad="D38"/>
<connect gate="G$1" pin="D39" pad="D39"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D40" pad="D40"/>
<connect gate="G$1" pin="D41" pad="D41"/>
<connect gate="G$1" pin="D42" pad="D42"/>
<connect gate="G$1" pin="D43" pad="D43"/>
<connect gate="G$1" pin="D44" pad="D44"/>
<connect gate="G$1" pin="D45" pad="D45"/>
<connect gate="G$1" pin="D46" pad="D46"/>
<connect gate="G$1" pin="D47" pad="D47"/>
<connect gate="G$1" pin="D48" pad="D48"/>
<connect gate="G$1" pin="D49" pad="D49"/>
<connect gate="G$1" pin="D5" pad="D5"/>
<connect gate="G$1" pin="D50" pad="D50"/>
<connect gate="G$1" pin="D51" pad="D51"/>
<connect gate="G$1" pin="D52" pad="D52"/>
<connect gate="G$1" pin="D53" pad="D53"/>
<connect gate="G$1" pin="D6" pad="D6"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="D9" pad="D9"/>
<connect gate="G$1" pin="GND" pad="GND_1 GND_2 GND_3"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="RESET" pad="RESET"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VIN" pad="VIN_1 VIN_2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Robotdyn"/>
<attribute name="MAXIMUM_PACKAGE_HIEGHT" value=" "/>
<attribute name="PARTREV" value="12/May/2017"/>
<attribute name="STANDARD" value="Manufacturer Recommendations"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EC11_ROTARY" prefix="S">
<description>Rotary Encoder Mechanical 15 Quadrature (Incremental) Vertical </description>
<gates>
<gate name="G$1" symbol="482016514001"/>
</gates>
<devices>
<device name="" package="SW_482016514001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Wurth Electronics"/>
<attribute name="MAXIMUM_PACKAGE_HEIGHT" value="26.9 mm"/>
<attribute name="PARTREV" value="001.000"/>
<attribute name="STANDARD" value="Manufacturer Recommendations"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="Power_Symbols">
<description>&lt;B&gt;Supply &amp; Ground symbols</description>
<packages>
</packages>
<symbols>
<symbol name="GND">
<description>Ground (GND) Arrow</description>
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="+5V">
<description>5 Volt (5V0) Bar</description>
<pin name="+5V" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="GND" prefix="SUPPLY" uservalue="yes">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt; - Ground (GND) Arrow</description>
<gates>
<gate name="G$1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name="">
<attribute name="CATEGORY" value="Supply"/>
<attribute name="VALUE" value="GND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="+5V" prefix="SUPPLY" uservalue="yes">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;  5 Volt (5V0) Bar</description>
<gates>
<gate name="G$1" symbol="+5V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name="">
<attribute name="CATEGORY" value="Supply"/>
<attribute name="VALUE" value="+5V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="CaptainBobSim Library, custom">
<packages>
<package name="IDC_40_2X20">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="LED_PUSH_7MM">
</package>
</packages>
<symbols>
<symbol name="IDC_40_PINH2X20">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
<pin name="21" direction="pas" function="dot"/>
<pin name="22" direction="pas" function="dot"/>
<pin name="23" direction="pas" function="dot"/>
<pin name="24" direction="pas" function="dot"/>
<pin name="25" direction="pas" function="dot"/>
<pin name="26" direction="pas" function="dot"/>
<pin name="27" direction="pas" function="dot"/>
<pin name="28" direction="pas" function="dot"/>
<pin name="29" direction="pas" function="dot"/>
<pin name="30" direction="pas" function="dot"/>
<pin name="31" direction="pas" function="dot"/>
<pin name="32" direction="pas" function="dot"/>
<pin name="33" direction="pas" function="dot"/>
<pin name="34" direction="pas" function="dot"/>
<pin name="35" direction="pas" function="dot"/>
<pin name="36" direction="pas" function="dot"/>
<pin name="37" direction="pas" function="dot"/>
<pin name="38" direction="pas" function="dot"/>
<pin name="39" direction="pas" function="dot"/>
<pin name="40" direction="pas" function="dot"/>
</symbol>
<symbol name="PUSH_LED">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="LED+" direction="out"/>
<pin name="LED-" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="IDC_40_PINHD-2X20" prefix="JP">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="IDC_40_PINH2X20"/>
</gates>
<devices>
<device name="" package="IDC_40_2X20">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="21" pad="21"/>
<connect gate="A" pin="22" pad="22"/>
<connect gate="A" pin="23" pad="23"/>
<connect gate="A" pin="24" pad="24"/>
<connect gate="A" pin="25" pad="25"/>
<connect gate="A" pin="26" pad="26"/>
<connect gate="A" pin="27" pad="27"/>
<connect gate="A" pin="28" pad="28"/>
<connect gate="A" pin="29" pad="29"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="30" pad="30"/>
<connect gate="A" pin="31" pad="31"/>
<connect gate="A" pin="32" pad="32"/>
<connect gate="A" pin="33" pad="33"/>
<connect gate="A" pin="34" pad="34"/>
<connect gate="A" pin="35" pad="35"/>
<connect gate="A" pin="36" pad="36"/>
<connect gate="A" pin="37" pad="37"/>
<connect gate="A" pin="38" pad="38"/>
<connect gate="A" pin="39" pad="39"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="40" pad="40"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED_PUSH_7MM" prefix="S">
<gates>
<gate name="G$1" symbol="PUSH_LED"/>
</gates>
<devices>
<device name="" package="LED_PUSH_7MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="LED+" pad="LED+"/>
<connect gate="G$1" pin="LED-" pad="LED-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="Resistor">
<description>&lt;B&gt;Resistors, Potentiometers, TrimPot</description>
<packages>
<package name="RESC1005X40">
<description>Chip, 1.05 X 0.54 X 0.40 mm body
&lt;p&gt;Chip package with body size 1.05 X 0.54 X 0.40 mm&lt;/p&gt;</description>
</package>
<package name="RESC1608X60">
<description>Chip, 1.60 X 0.82 X 0.60 mm body
&lt;p&gt;Chip package with body size 1.60 X 0.82 X 0.60 mm&lt;/p&gt;</description>
</package>
<package name="RESC2012X65">
<description>Chip, 2.00 X 1.25 X 0.65 mm body
&lt;p&gt;Chip package with body size 2.00 X 1.25 X 0.65 mm&lt;/p&gt;</description>
</package>
<package name="RESC3216X70">
<description>Chip, 3.20 X 1.60 X 0.70 mm body
&lt;p&gt;Chip package with body size 3.20 X 1.60 X 0.70 mm&lt;/p&gt;</description>
</package>
<package name="RESC3224X71">
<description>Chip, 3.20 X 2.49 X 0.71 mm body
&lt;p&gt;Chip package with body size 3.20 X 2.49 X 0.71 mm&lt;/p&gt;</description>
</package>
<package name="RESC5025X71">
<description>Chip, 5.00 X 2.50 X 0.71 mm body
&lt;p&gt;Chip package with body size 5.00 X 2.50 X 0.71 mm&lt;/p&gt;</description>
</package>
<package name="RESC6332X71">
<description>Chip, 6.30 X 3.20 X 0.71 mm body
&lt;p&gt;Chip package with body size 6.30 X 3.20 X 0.71 mm&lt;/p&gt;</description>
</package>
<package name="RESAD1176W63L850D250B">
<description>AXIAL Resistor, 11.76 mm pitch, 8.5 mm body length, 2.5 mm body diameter
&lt;p&gt;AXIAL Resistor package with 11.76 mm pitch, 0.63 mm lead diameter, 8.5 mm body length and 2.5 mm body diameter&lt;/p&gt;</description>
</package>
<package name="RESMELF3515">
<description>MELF, 3.50 mm length, 1.52 mm diameter
&lt;p&gt;MELF Resistor package with 3.50 mm length and 1.52 mm diameter&lt;/p&gt;</description>
</package>
<package name="RESMELF2014">
<description>MELF, 2.00 mm length, 1.40 mm diameter
&lt;p&gt;MELF Resistor package with 2.00 mm length and 1.40 mm diameter&lt;/p&gt;</description>
</package>
<package name="RESMELF5924">
<description>MELF, 5.90 mm length, 2.45 mm diameter
&lt;p&gt;MELF Resistor package with 5.90 mm length and 2.45 mm diameter&lt;/p&gt;</description>
</package>
<package name="RESMELF3218">
<description>MELF, 3.20 mm length, 1.80 mm diameter
&lt;p&gt;MELF Resistor package with 3.20 mm length and 1.80 mm diameter&lt;/p&gt;</description>
</package>
<package name="RESAD724W46L381D178B">
<description>Axial Resistor, 7.24 mm pitch, 3.81 mm body length, 1.78 mm body diameter
&lt;p&gt;Axial Resistor package with 7.24 mm pitch (lead spacing), 0.46 mm lead diameter, 3.81 mm body length and 1.78 mm body diameter&lt;/p&gt;</description>
</package>
</packages>
<symbols>
<symbol name="R-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="R-US" prefix="R" uservalue="yes">
<description>&lt;B&gt;Resistor Fixed - ANSI</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="CHIP-0402(1005-METRIC)" package="RESC1005X40">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Resistor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="RATING" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value=""/>
</technology>
</technologies>
</device>
<device name="CHIP-0603(1608-METRIC)" package="RESC1608X60">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Resistor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="RATING" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value=""/>
</technology>
</technologies>
</device>
<device name="CHIP-0805(2012-METRIC)" package="RESC2012X65">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Resistor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="RATING" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value=""/>
</technology>
</technologies>
</device>
<device name="CHIP-1206(3216-METRIC)" package="RESC3216X70">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Resistor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="RATING" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value=""/>
</technology>
</technologies>
</device>
<device name="CHIP-1210(3225-METRIC)" package="RESC3224X71">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Resistor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="RATING" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value=""/>
</technology>
</technologies>
</device>
<device name="CHIP-2010(5025-METRIC)" package="RESC5025X71">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Resistor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="RATING" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value=""/>
</technology>
</technologies>
</device>
<device name="CHIP-2512(6332-METRIC)" package="RESC6332X71">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Resistor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="RATING" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value=""/>
</technology>
</technologies>
</device>
<device name="AXIAL-11.7MM-PITCH" package="RESAD1176W63L850D250B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Resistor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="RATING" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value=""/>
</technology>
</technologies>
</device>
<device name="MELF(3515-METRIC)" package="RESMELF3515">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Resistor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="RATING" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value=""/>
</technology>
</technologies>
</device>
<device name="MELF(2014-METRIC)" package="RESMELF2014">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Resistor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="RATING" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value=""/>
</technology>
</technologies>
</device>
<device name="MELF(5924-METRIC)" package="RESMELF5924">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Resistor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="RATING" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value=""/>
</technology>
</technologies>
</device>
<device name="MELF(3218-METRIC)" package="RESMELF3218">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Resistor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="RATING" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value=""/>
</technology>
</technologies>
</device>
<device name="AXIAL-7.2MM-PITCH" package="RESAD724W46L381D178B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Resistor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="RATING" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value=""/>
</technology>
</technologies>
</device>
</devices>
<spice>
<pinmapping spiceprefix="R">
<pinmap gate="G$1" pin="1" pinorder="1"/>
<pinmap gate="G$1" pin="2" pinorder="2"/>
</pinmapping>
</spice>
</deviceset>
</devicesets>
</library>
<library name="Connector">
<description>&lt;b&gt;Pin Headers,Terminal blocks, D-Sub, Backplane, FFC/FPC, Socket</description>
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="PINHD3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PINHD-1X3" prefix="JP">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD3"/>
</gates>
<devices>
<device name="" package="1X03">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CATEGORY" value="Headers"/>
<attribute name="DESCRIPTION" value="Header, Straight, 3 Position"/>
<attribute name="MANUFACTURER" value="Generic"/>
<attribute name="MPN" value="Generic"/>
<attribute name="OPERATING_TEMPERATURE" value="Generic"/>
<attribute name="PART_STATUS" value="Active"/>
<attribute name="PITCH" value="0.100&quot; (2.54mm)"/>
<attribute name="ROHS_COMPLIANCE" value="Generic"/>
<attribute name="SERIES" value="Generic"/>
<attribute name="SUB-CATEGORY" value="Headers, Male Pins"/>
<attribute name="TYPE" value="Board to Board or Cable, Unshrouded, Through Hole, Straight"/>
</technology>
</technologies>
</device>
<device name="/90" package="1X03/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CATEGORY" value="Headers"/>
<attribute name="DESCRIPTION" value="Header, Right Angle, 3 Position"/>
<attribute name="MANUFACTURER" value="Generic"/>
<attribute name="MPN" value="Generic"/>
<attribute name="OPERATING_TEMPERATURE" value="Generic"/>
<attribute name="PART_STATUS" value="Active"/>
<attribute name="PITCH" value="0.100&quot; (2.54mm)"/>
<attribute name="ROHS_COMPLIANCE" value="Generic"/>
<attribute name="SERIES" value="Generic"/>
<attribute name="SUB-CATEGORY" value="Headers, Male Pins"/>
<attribute name="TYPE" value="Board to Board or Cable, Unshrouded, Through Hole, Right Angle"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="PINHD2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PINHD-1X2" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD2"/>
</gates>
<devices>
<device name="" package="1X02">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="POPULARITY" value="98"/>
</technology>
</technologies>
</device>
<device name="/90" package="1X02/90">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="POPULARITY" value="24"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="SUPPLY7" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="SUPPLY26" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="SUPPLY30" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="SUPPLY31" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="SUPPLY32" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="SUPPLY33" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="SUPPLY34" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="SUPPLY35" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="ENT1" library="CaptainBobSim Library, custom" deviceset="LED_PUSH_7MM" device=""/>
<part name="SUPPLY36" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="CLR1" library="CaptainBobSim Library, custom" deviceset="LED_PUSH_7MM" device=""/>
<part name="SUPPLY37" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="MENU1" library="CaptainBobSim Library, custom" deviceset="LED_PUSH_7MM" device=""/>
<part name="SUPPLY38" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="-D-&gt;1" library="CaptainBobSim Library, custom" deviceset="LED_PUSH_7MM" device=""/>
<part name="SUPPLY39" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="DN1" library="CaptainBobSim Library, custom" deviceset="LED_PUSH_7MM" device=""/>
<part name="SUPPLY40" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="UP1" library="CaptainBobSim Library, custom" deviceset="LED_PUSH_7MM" device=""/>
<part name="SUPPLY41" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="SUPPLY42" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="SUPPLY43" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="SUPPLY44" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="SUPPLY45" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="SUPPLY46" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="ENC3" library="ALPS Dual Library" deviceset="ALPS_EC11EBB24C03" device="ALPS_EC11EBB24C03_0_0"/>
<part name="SUPPLY47" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="SUPPLY48" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="ENC4" library="ALPS Dual Library" deviceset="ALPS_EC11EBB24C03" device="ALPS_EC11EBB24C03_0_0"/>
<part name="SUPPLY49" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="SUPPLY50" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="ARDUINO_PRO_MEGA" library="SnapEDA Library" deviceset="MEGA_PRO_EMBED_CH340G_/_ATMEGA2560" device=""/>
<part name="SUPPLY51" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="SUPPLY52" library="Power_Symbols" deviceset="+5V" device="" value="+5V"/>
<part name="SUPPLY53" library="Power_Symbols" deviceset="+5V" device="" value="+5V"/>
<part name="OUTBOUND" library="CaptainBobSim Library, custom" deviceset="IDC_40_PINHD-2X20" device=""/>
<part name="COM" library="SnapEDA Library" deviceset="EC11_ROTARY" device=""/>
<part name="NAV" library="SnapEDA Library" deviceset="EC11_ROTARY" device=""/>
<part name="COM_SWAP" library="CaptainBobSim Library, custom" deviceset="LED_PUSH_7MM" device=""/>
<part name="NAV_SWAP" library="CaptainBobSim Library, custom" deviceset="LED_PUSH_7MM" device=""/>
<part name="CDI1" library="CaptainBobSim Library, custom" deviceset="LED_PUSH_7MM" device=""/>
<part name="OBS1" library="CaptainBobSim Library, custom" deviceset="LED_PUSH_7MM" device=""/>
<part name="MSG1" library="CaptainBobSim Library, custom" deviceset="LED_PUSH_7MM" device=""/>
<part name="FPL1" library="CaptainBobSim Library, custom" deviceset="LED_PUSH_7MM" device=""/>
<part name="PROC1" library="CaptainBobSim Library, custom" deviceset="LED_PUSH_7MM" device=""/>
<part name="IDC_40A" library="CaptainBobSim Library, custom" deviceset="IDC_40_PINHD-2X20" device=""/>
<part name="SUPPLY54" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="SUPPLY55" library="Power_Symbols" deviceset="+5V" device="" value="+5V"/>
<part name="SUPPLY56" library="Power_Symbols" deviceset="+5V" device="" value="+5V"/>
<part name="BACKLIGHT" library="Connector" deviceset="PINHD-1X3" device=""/>
<part name="SUPPLY57" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="EXT_BKLT" library="pinhead" deviceset="PINHD-1X2" device=""/>
<part name="SUPPLY58" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="R2" library="Resistor" deviceset="R-US" device="AXIAL-7.2MM-PITCH" technology="_"/>
<part name="SUPPLY59" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="R3" library="Resistor" deviceset="R-US" device="AXIAL-7.2MM-PITCH" technology="_"/>
<part name="SUPPLY60" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="R4" library="Resistor" deviceset="R-US" device="AXIAL-7.2MM-PITCH" technology="_"/>
<part name="SUPPLY61" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
<part name="R1" library="Resistor" deviceset="R-US" device="AXIAL-7.2MM-PITCH" technology="_"/>
<part name="SUPPLY62" library="Power_Symbols" deviceset="GND" device="" value="GND"/>
</parts>
<sheets>
<sheet>
<plain>
<text>Changelog
V1.0 Initial Design 
V1.1 Redo resistor traces, pinout</text>
<text>Changelog
V1.0 Initial Design (Date)</text>
</plain>
<busses>
</busses>
<nets>
<net name="GND">
<segment>
<pinref part="SUPPLY7" gate="G$1" pin="GND"/>
<pinref part="COM_SWAP" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="SUPPLY26" gate="G$1" pin="GND"/>
<pinref part="NAV_SWAP" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="SUPPLY36" gate="G$1" pin="GND"/>
<pinref part="ENT1" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="SUPPLY37" gate="G$1" pin="GND"/>
<pinref part="CLR1" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="SUPPLY38" gate="G$1" pin="GND"/>
<pinref part="MENU1" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="SUPPLY39" gate="G$1" pin="GND"/>
<pinref part="-D-&gt;1" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="SUPPLY40" gate="G$1" pin="GND"/>
<pinref part="DN1" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="SUPPLY41" gate="G$1" pin="GND"/>
<pinref part="UP1" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="SUPPLY47" gate="G$1" pin="GND"/>
<pinref part="ENC3" gate="G$0" pin="C"/>
<pinref part="ENC3" gate="G$0" pin="C'"/>
</segment>
<segment>
<pinref part="SUPPLY48" gate="G$1" pin="GND"/>
<pinref part="ENC3" gate="G$0" pin="E"/>
</segment>
<segment>
<pinref part="SUPPLY50" gate="G$1" pin="GND"/>
<pinref part="ENC4" gate="G$0" pin="E"/>
</segment>
<segment>
<pinref part="SUPPLY49" gate="G$1" pin="GND"/>
<pinref part="ENC4" gate="G$0" pin="C"/>
<pinref part="ENC4" gate="G$0" pin="C'"/>
</segment>
<segment>
<pinref part="SUPPLY42" gate="G$1" pin="GND"/>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="SUPPLY51" gate="G$1" pin="GND"/>
<pinref part="OUTBOUND" gate="A" pin="1"/>
</segment>
<segment>
<pinref part="SUPPLY44" gate="G$1" pin="GND"/>
<pinref part="COM" gate="G$1" pin="C"/>
</segment>
<segment>
<pinref part="COM" gate="G$1" pin="2"/>
<pinref part="SUPPLY43" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="NAV" gate="G$1" pin="C"/>
<pinref part="SUPPLY46" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="NAV" gate="G$1" pin="2"/>
<pinref part="SUPPLY45" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="SUPPLY30" gate="G$1" pin="GND"/>
<pinref part="CDI1" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="SUPPLY31" gate="G$1" pin="GND"/>
<pinref part="OBS1" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="SUPPLY32" gate="G$1" pin="GND"/>
<pinref part="MSG1" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="SUPPLY33" gate="G$1" pin="GND"/>
<pinref part="FPL1" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="SUPPLY35" gate="G$1" pin="GND"/>
<pinref part="PROC1" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="SUPPLY54" gate="G$1" pin="GND"/>
<pinref part="IDC_40A" gate="A" pin="1"/>
</segment>
<segment>
<pinref part="SUPPLY57" gate="G$1" pin="GND"/>
<pinref part="BACKLIGHT" gate="A" pin="1"/>
</segment>
<segment>
<pinref part="EXT_BKLT" gate="G$1" pin="1"/>
<pinref part="SUPPLY58" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="R2" gate="G$1" pin="1"/>
<pinref part="SUPPLY59" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="R3" gate="G$1" pin="1"/>
<pinref part="SUPPLY60" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="R4" gate="G$1" pin="1"/>
<pinref part="SUPPLY61" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="R1" gate="G$1" pin="1"/>
<pinref part="SUPPLY62" gate="G$1" pin="GND"/>
</segment>
</net>
<net name="CDI">
<segment>
<pinref part="CDI1" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="OUTBOUND" gate="A" pin="17"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D34"/>
</segment>
</net>
<net name="FPL">
<segment>
<pinref part="FPL1" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="OUTBOUND" gate="A" pin="20"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D37"/>
</segment>
</net>
<net name="MSG">
<segment>
<pinref part="MSG1" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="OUTBOUND" gate="A" pin="19"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D36"/>
</segment>
</net>
<net name="OBS">
<segment>
<pinref part="OBS1" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="OUTBOUND" gate="A" pin="18"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D35"/>
</segment>
</net>
<net name="PROC">
<segment>
<pinref part="PROC1" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="OUTBOUND" gate="A" pin="22"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D39"/>
</segment>
</net>
<net name="ENT">
<segment>
<pinref part="ENT1" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="OUTBOUND" gate="A" pin="28"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="A6"/>
</segment>
</net>
<net name="CLR">
<segment>
<pinref part="CLR1" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="OUTBOUND" gate="A" pin="29"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="A7"/>
</segment>
</net>
<net name="MENU">
<segment>
<pinref part="MENU1" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="OUTBOUND" gate="A" pin="30"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="A10"/>
</segment>
</net>
<net name="-D-">
<segment>
<pinref part="-D-&gt;1" gate="G$1" pin="3"/>
</segment>
</net>
<net name="DN">
<segment>
<pinref part="DN1" gate="G$1" pin="3"/>
</segment>
</net>
<net name="UP">
<segment>
<pinref part="UP1" gate="G$1" pin="3"/>
</segment>
</net>
<net name="+5V">
<segment>
<pinref part="SUPPLY52" gate="G$1" pin="+5V"/>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="5V"/>
</segment>
<segment>
<pinref part="SUPPLY53" gate="G$1" pin="+5V"/>
<pinref part="OUTBOUND" gate="A" pin="2"/>
</segment>
<segment>
<pinref part="SUPPLY55" gate="G$1" pin="+5V"/>
<pinref part="IDC_40A" gate="A" pin="2"/>
</segment>
<segment>
<pinref part="SUPPLY56" gate="G$1" pin="+5V"/>
<pinref part="BACKLIGHT" gate="A" pin="3"/>
</segment>
</net>
<net name="COM_SWAP">
<segment>
<pinref part="COM_SWAP" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="OUTBOUND" gate="A" pin="3"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D10"/>
</segment>
</net>
<net name="COM_B">
<segment>
<pinref part="COM" gate="G$1" pin="B"/>
</segment>
<segment>
<pinref part="OUTBOUND" gate="A" pin="6"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D44"/>
</segment>
</net>
<net name="COM_PRESS">
<segment>
<pinref part="COM" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="OUTBOUND" gate="A" pin="7"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D45"/>
</segment>
</net>
<net name="NAV_SWAP">
<segment>
<pinref part="NAV_SWAP" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="OUTBOUND" gate="A" pin="8"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D46"/>
</segment>
</net>
<net name="VNAV">
<segment>
</segment>
<segment>
<pinref part="OUTBOUND" gate="A" pin="21"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D38"/>
</segment>
</net>
<net name="R_ROUGHB">
<segment>
<pinref part="ENC4" gate="G$0" pin="B'"/>
</segment>
<segment>
<pinref part="OUTBOUND" gate="A" pin="26"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D43"/>
</segment>
</net>
<net name="COM_A">
<segment>
<pinref part="COM" gate="G$1" pin="A"/>
</segment>
<segment>
<pinref part="OUTBOUND" gate="A" pin="5"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D12"/>
</segment>
</net>
<net name="COM_POWER">
<segment>
<pinref part="OUTBOUND" gate="A" pin="4"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D11"/>
</segment>
</net>
<net name="NAV_A">
<segment>
<pinref part="OUTBOUND" gate="A" pin="9"/>
</segment>
<segment>
<pinref part="NAV" gate="G$1" pin="A"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D47"/>
</segment>
</net>
<net name="NAV_B">
<segment>
<pinref part="OUTBOUND" gate="A" pin="10"/>
</segment>
<segment>
<pinref part="NAV" gate="G$1" pin="B"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D48"/>
</segment>
</net>
<net name="NAV_PRESS">
<segment>
<pinref part="OUTBOUND" gate="A" pin="11"/>
</segment>
<segment>
<pinref part="NAV" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D49"/>
</segment>
</net>
<net name="L_FINEA">
<segment>
<pinref part="OUTBOUND" gate="A" pin="12"/>
</segment>
<segment>
<pinref part="ENC3" gate="G$0" pin="A"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D50"/>
</segment>
</net>
<net name="L_FINEB">
<segment>
<pinref part="OUTBOUND" gate="A" pin="13"/>
</segment>
<segment>
<pinref part="ENC3" gate="G$0" pin="B"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D51"/>
</segment>
</net>
<net name="L_ROUGHA">
<segment>
<pinref part="OUTBOUND" gate="A" pin="14"/>
</segment>
<segment>
<pinref part="ENC3" gate="G$0" pin="A'"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D52"/>
</segment>
</net>
<net name="L_ROUGHB">
<segment>
<pinref part="OUTBOUND" gate="A" pin="15"/>
</segment>
<segment>
<pinref part="ENC3" gate="G$0" pin="B'"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D53"/>
</segment>
</net>
<net name="L_PRESS">
<segment>
<pinref part="OUTBOUND" gate="A" pin="16"/>
</segment>
<segment>
<pinref part="ENC3" gate="G$0" pin="D"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D33"/>
</segment>
</net>
<net name="R_FINEA">
<segment>
<pinref part="ENC4" gate="G$0" pin="A"/>
</segment>
<segment>
<pinref part="OUTBOUND" gate="A" pin="23"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D40"/>
</segment>
</net>
<net name="R_FINEB">
<segment>
<pinref part="ENC4" gate="G$0" pin="B"/>
</segment>
<segment>
<pinref part="OUTBOUND" gate="A" pin="24"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D41"/>
</segment>
</net>
<net name="R_ROUGHA">
<segment>
<pinref part="ENC4" gate="G$0" pin="A'"/>
</segment>
<segment>
<pinref part="OUTBOUND" gate="A" pin="25"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D42"/>
</segment>
</net>
<net name="COM_VOL">
<segment>
<pinref part="OUTBOUND" gate="A" pin="39"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="A14"/>
</segment>
</net>
<net name="NAV_VOL">
<segment>
<pinref part="OUTBOUND" gate="A" pin="40"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="A15"/>
</segment>
</net>
<net name="R_PRESS">
<segment>
<pinref part="ENC4" gate="G$0" pin="D"/>
</segment>
<segment>
<pinref part="OUTBOUND" gate="A" pin="27"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="A5"/>
</segment>
</net>
<net name="VIN">
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="VIN"/>
</segment>
</net>
<net name="RNG_DN">
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="A12"/>
</segment>
<segment>
<pinref part="OUTBOUND" gate="A" pin="32"/>
</segment>
</net>
<net name="RNG_UP">
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="A13"/>
</segment>
<segment>
<pinref part="OUTBOUND" gate="A" pin="33"/>
</segment>
</net>
<net name="DIRECT">
<segment>
<pinref part="OUTBOUND" gate="A" pin="31"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="A11"/>
</segment>
</net>
<net name="A_D2">
<segment>
<pinref part="IDC_40A" gate="A" pin="3"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D2"/>
</segment>
</net>
<net name="A_D4">
<segment>
<pinref part="IDC_40A" gate="A" pin="5"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D4"/>
</segment>
</net>
<net name="A_D6">
<segment>
<pinref part="IDC_40A" gate="A" pin="23"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D6"/>
</segment>
</net>
<net name="A_D8">
<segment>
<pinref part="IDC_40A" gate="A" pin="25"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D8"/>
</segment>
</net>
<net name="A_D14">
<segment>
<pinref part="IDC_40A" gate="A" pin="7"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D14"/>
</segment>
</net>
<net name="A_D16">
<segment>
<pinref part="IDC_40A" gate="A" pin="9"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D16"/>
</segment>
</net>
<net name="A_D18">
<segment>
<pinref part="IDC_40A" gate="A" pin="11"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D18"/>
</segment>
</net>
<net name="A_D20">
<segment>
<pinref part="IDC_40A" gate="A" pin="13"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D20"/>
</segment>
</net>
<net name="A_D22">
<segment>
<pinref part="IDC_40A" gate="A" pin="15"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D22"/>
</segment>
</net>
<net name="A_D24">
<segment>
<pinref part="IDC_40A" gate="A" pin="22"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D24"/>
</segment>
</net>
<net name="A_D28">
<segment>
<pinref part="IDC_40A" gate="A" pin="30"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D28"/>
</segment>
</net>
<net name="A_D30">
<segment>
<pinref part="IDC_40A" gate="A" pin="32"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D30"/>
</segment>
</net>
<net name="A_D32">
<segment>
<pinref part="IDC_40A" gate="A" pin="34"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D32"/>
</segment>
</net>
<net name="A_D26">
<segment>
<pinref part="IDC_40A" gate="A" pin="28"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D26"/>
</segment>
</net>
<net name="A_D3">
<segment>
<pinref part="IDC_40A" gate="A" pin="4"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D3"/>
</segment>
</net>
<net name="A_D5">
<segment>
<pinref part="IDC_40A" gate="A" pin="6"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D5"/>
</segment>
</net>
<net name="A_D7">
<segment>
<pinref part="IDC_40A" gate="A" pin="24"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D7"/>
</segment>
</net>
<net name="A_D9">
<segment>
<pinref part="IDC_40A" gate="A" pin="26"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D9"/>
</segment>
</net>
<net name="A_D15">
<segment>
<pinref part="IDC_40A" gate="A" pin="8"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D15"/>
</segment>
</net>
<net name="A_D17">
<segment>
<pinref part="IDC_40A" gate="A" pin="10"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D17"/>
</segment>
</net>
<net name="A_D19">
<segment>
<pinref part="IDC_40A" gate="A" pin="12"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D19"/>
</segment>
</net>
<net name="A_D21">
<segment>
<pinref part="IDC_40A" gate="A" pin="14"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D21"/>
</segment>
</net>
<net name="A_D23">
<segment>
<pinref part="IDC_40A" gate="A" pin="21"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D23"/>
</segment>
</net>
<net name="A_D25">
<segment>
<pinref part="IDC_40A" gate="A" pin="27"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D25"/>
</segment>
</net>
<net name="A_D27">
<segment>
<pinref part="IDC_40A" gate="A" pin="29"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D27"/>
</segment>
</net>
<net name="A_D29">
<segment>
<pinref part="IDC_40A" gate="A" pin="31"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D29"/>
</segment>
</net>
<net name="A_D31">
<segment>
<pinref part="IDC_40A" gate="A" pin="33"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="D31"/>
</segment>
</net>
<net name="A_D33">
<segment>
<pinref part="IDC_40A" gate="A" pin="35"/>
</segment>
</net>
<net name="A_A1">
<segment>
<pinref part="IDC_40A" gate="A" pin="17"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="A1"/>
</segment>
</net>
<net name="A_A3">
<segment>
<pinref part="IDC_40A" gate="A" pin="19"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="A3"/>
</segment>
</net>
<net name="A_A5">
<segment>
<pinref part="IDC_40A" gate="A" pin="36"/>
</segment>
</net>
<net name="A_A7">
<segment>
<pinref part="IDC_40A" gate="A" pin="38"/>
</segment>
</net>
<net name="A_A0">
<segment>
<pinref part="IDC_40A" gate="A" pin="16"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="A0"/>
</segment>
</net>
<net name="A_A2">
<segment>
<pinref part="IDC_40A" gate="A" pin="18"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="A2"/>
</segment>
</net>
<net name="A_A4">
<segment>
<pinref part="IDC_40A" gate="A" pin="20"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="A4"/>
</segment>
</net>
<net name="A_A6">
<segment>
<pinref part="IDC_40A" gate="A" pin="37"/>
</segment>
</net>
<net name="A_A8">
<segment>
<pinref part="IDC_40A" gate="A" pin="39"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="A8"/>
</segment>
</net>
<net name="A_A9">
<segment>
<pinref part="IDC_40A" gate="A" pin="40"/>
</segment>
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="A9"/>
</segment>
</net>
<net name="A_AREF">
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="AREF"/>
</segment>
</net>
<net name="A_RX">
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="RX"/>
</segment>
</net>
<net name="A_3V3">
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="3V3"/>
</segment>
</net>
<net name="A_RST">
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="RST"/>
</segment>
</net>
<net name="A_TX">
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="TX"/>
</segment>
</net>
<net name="A_MOSI">
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="MOSI"/>
</segment>
</net>
<net name="A_MISO">
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="MISO"/>
</segment>
</net>
<net name="A_SCK">
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="SCK"/>
</segment>
</net>
<net name="A_RESET">
<segment>
<pinref part="ARDUINO_PRO_MEGA" gate="G$1" pin="RESET"/>
</segment>
</net>
<net name="N$13">
<segment>
<pinref part="BACKLIGHT" gate="A" pin="2"/>
<pinref part="EXT_BKLT" gate="G$1" pin="2"/>
<pinref part="COM_SWAP" gate="G$1" pin="LED+"/>
<pinref part="NAV_SWAP" gate="G$1" pin="LED+"/>
<pinref part="CDI1" gate="G$1" pin="LED+"/>
<pinref part="OBS1" gate="G$1" pin="LED+"/>
<pinref part="CDI1" gate="G$1" pin="4"/>
<pinref part="MSG1" gate="G$1" pin="LED+"/>
<pinref part="FPL1" gate="G$1" pin="LED+"/>
<pinref part="PROC1" gate="G$1" pin="LED+"/>
<pinref part="ENT1" gate="G$1" pin="LED+"/>
<pinref part="CLR1" gate="G$1" pin="LED+"/>
<pinref part="MENU1" gate="G$1" pin="LED+"/>
<pinref part="-D-&gt;1" gate="G$1" pin="LED+"/>
<pinref part="DN1" gate="G$1" pin="LED+"/>
<pinref part="UP1" gate="G$1" pin="LED+"/>
</segment>
</net>
<net name="N$23">
<segment>
<pinref part="NAV_SWAP" gate="G$1" pin="LED-"/>
<pinref part="COM_SWAP" gate="G$1" pin="LED-"/>
<pinref part="CDI1" gate="G$1" pin="LED-"/>
<pinref part="OBS1" gate="G$1" pin="LED-"/>
<pinref part="R1" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$24">
<segment>
<pinref part="MSG1" gate="G$1" pin="LED-"/>
<pinref part="R2" gate="G$1" pin="2"/>
<pinref part="FPL1" gate="G$1" pin="LED-"/>
<pinref part="PROC1" gate="G$1" pin="LED-"/>
</segment>
</net>
<net name="N$34">
<segment>
<pinref part="ENT1" gate="G$1" pin="LED-"/>
<pinref part="R3" gate="G$1" pin="2"/>
<pinref part="CLR1" gate="G$1" pin="LED-"/>
<pinref part="MENU1" gate="G$1" pin="LED-"/>
</segment>
</net>
<net name="N$35">
<segment>
<pinref part="UP1" gate="G$1" pin="LED-"/>
<pinref part="R4" gate="G$1" pin="2"/>
<pinref part="DN1" gate="G$1" pin="LED-"/>
<pinref part="-D-&gt;1" gate="G$1" pin="LED-"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
